<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<library>
<packages>
<package name="254MIL_GND_TIE">
</package>
<package name="SC70-6L">
<description>&lt;b&gt;SC-70 Package&lt;/b&gt;</description>
</package>
<package name="DIL14">
<description>&lt;b&gt;Dual In Line Package&lt;/b&gt;</description>
</package>
<package name="QFN16-4X4">
<description>&lt;b&gt;16-Lead Plastic Quad Flat, No Lead Package (ML) - 4x4x0.9mm Body [QFN]&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
</package>
<package name="PAIR-1X6-SMT">
<description>TE Connectivity 5-146128-4

&lt;p&gt;
(2) 6-pin male SMT headers</description>
</package>
<package name="RJ45-VERT">
<description>TE 5520259-4 -- RJ45, vertical mount

&lt;p&gt;
http://www.te.com/catalog/pn/en/5520259-4?RQPN=5520259-4</description>
</package>
</packages>
<symbols>
<symbol name="254MIL_GND_TIE">
<pin name="P$1"/>
<pin name="P$2"/>
</symbol>
<symbol name="IC">
<pin name="VCC" direction="pwr"/>
<pin name="ENABLE" direction="in"/>
<pin name="GND@2" direction="pwr"/>
<pin name="BUS1"/>
<pin name="GND@5" direction="pwr"/>
<pin name="BUS2"/>
</symbol>
<symbol name="PIC16F688">
<pin name="VDD" direction="pwr"/>
<pin name="RA4/AN3/!T1G!/OSC2/CLKOUT"/>
<pin name="RA3/!MCLR!/VPP"/>
<pin name="RA5/T1CKI/OSC1/CLKIN"/>
<pin name="RA0/AN0/C1IN+/ICSPDAT/ULPWU"/>
<pin name="RA1/AN1/C1IN-/VREF/ICSPCLK"/>
<pin name="RA2/AN2/T0CKI/INT/C1OUT"/>
<pin name="RC2/AN6"/>
<pin name="RC1/AN5/C2IN"/>
<pin name="RC0/AN4/C2IN+"/>
<pin name="RC5/RX/DT"/>
<pin name="RC4/C2OUT/TX/CK"/>
<pin name="RC3/AN7"/>
<pin name="VSS" direction="pwr"/>
</symbol>
<symbol name="MVAL">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="M">
<pin name="S" direction="pas"/>
</symbol>
<symbol name="RJ45">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
<pin name="P$4"/>
<pin name="P$5"/>
<pin name="P$6"/>
<pin name="P$7"/>
<pin name="P$8"/>
</symbol>
<symbol name="JACK8">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="254MIL_GND_TIE" prefix="PT">
<description>Package for connecting a 254mil ground net to another.</description>
<gates>
<gate name="G$1" symbol="254MIL_GND_TIE"/>
</gates>
<devices>
<device name="" package="254MIL_GND_TIE">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LTC4311" prefix="U">
<description>Low Voltage I2C/SMBus Accelerator

http://www.linear.com/product/LTC4311</description>
<gates>
<gate name="G$1" symbol="IC"/>
</gates>
<devices>
<device name="" package="SC70-6L">
<connects>
<connect gate="G$1" pin="BUS1" pad="6"/>
<connect gate="G$1" pin="BUS2" pad="4"/>
<connect gate="G$1" pin="ENABLE" pad="3"/>
<connect gate="G$1" pin="GND@2" pad="2"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PIC16F688" prefix="IC">
<description>&lt;b&gt;14-Pin Flash-Based, 8-Bit CMOS Microcontrollers with nanoWatt Technology&lt;/b&gt;&lt;p&gt;
Source: http://ww1.microchip.com/downloads/en/DeviceDoc/41203E.pdf</description>
<gates>
<gate name="G$1" symbol="PIC16F688"/>
</gates>
<devices>
<device name="QFN" package="QFN16-4X4">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1IN+/ICSPDAT/ULPWU" pad="12"/>
<connect gate="G$1" pin="RA1/AN1/C1IN-/VREF/ICSPCLK" pad="11"/>
<connect gate="G$1" pin="RA2/AN2/T0CKI/INT/C1OUT" pad="10"/>
<connect gate="G$1" pin="RA3/!MCLR!/VPP" pad="3"/>
<connect gate="G$1" pin="RA4/AN3/!T1G!/OSC2/CLKOUT" pad="2"/>
<connect gate="G$1" pin="RA5/T1CKI/OSC1/CLKIN" pad="1"/>
<connect gate="G$1" pin="RC0/AN4/C2IN+" pad="9"/>
<connect gate="G$1" pin="RC1/AN5/C2IN" pad="8"/>
<connect gate="G$1" pin="RC2/AN6" pad="7"/>
<connect gate="G$1" pin="RC3/AN7" pad="6"/>
<connect gate="G$1" pin="RC4/C2OUT/TX/CK" pad="5"/>
<connect gate="G$1" pin="RC5/RX/DT" pad="4"/>
<connect gate="G$1" pin="VDD" pad="16"/>
<connect gate="G$1" pin="VSS" pad="13"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value=""/>
<attribute name="MPN" value="PIC16F688-I/ML"/>
<attribute name="OC_FARNELL" value="1579588"/>
<attribute name="OC_NEWARK" value="56K7280"/>
</technology>
</technologies>
</device>
<device name="DIP" package="DIL14">
<connects>
<connect gate="G$1" pin="RA0/AN0/C1IN+/ICSPDAT/ULPWU" pad="13"/>
<connect gate="G$1" pin="RA1/AN1/C1IN-/VREF/ICSPCLK" pad="12"/>
<connect gate="G$1" pin="RA2/AN2/T0CKI/INT/C1OUT" pad="11"/>
<connect gate="G$1" pin="RA3/!MCLR!/VPP" pad="4"/>
<connect gate="G$1" pin="RA4/AN3/!T1G!/OSC2/CLKOUT" pad="3"/>
<connect gate="G$1" pin="RA5/T1CKI/OSC1/CLKIN" pad="2"/>
<connect gate="G$1" pin="RC0/AN4/C2IN+" pad="10"/>
<connect gate="G$1" pin="RC1/AN5/C2IN" pad="9"/>
<connect gate="G$1" pin="RC2/AN6" pad="8"/>
<connect gate="G$1" pin="RC3/AN7" pad="7"/>
<connect gate="G$1" pin="RC4/C2OUT/TX/CK" pad="6"/>
<connect gate="G$1" pin="RC5/RX/DT" pad="5"/>
<connect gate="G$1" pin="VDD" pad="1"/>
<connect gate="G$1" pin="VSS" pad="14"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="PAIR-1X6" prefix="X">
<description>TE Connectivity 5-146128-4

&lt;p&gt;
(2) 6-pin male SMT headers

&lt;p&gt;
http://www.te.com/catalog/pn/en/5-146128-4</description>
<gates>
<gate name="1" symbol="MVAL"/>
<gate name="3" symbol="M"/>
<gate name="4" symbol="M"/>
<gate name="5" symbol="M"/>
<gate name="6" symbol="M"/>
<gate name="7" symbol="M"/>
<gate name="8" symbol="M"/>
<gate name="9" symbol="M"/>
<gate name="10" symbol="M"/>
<gate name="11" symbol="M"/>
<gate name="12" symbol="M"/>
<gate name="2" symbol="M"/>
</gates>
<devices>
<device name="" package="PAIR-1X6-SMT">
<connects>
<connect gate="1" pin="S" pad="P$1"/>
<connect gate="10" pin="S" pad="P$10"/>
<connect gate="11" pin="S" pad="P$11"/>
<connect gate="12" pin="S" pad="P$12"/>
<connect gate="2" pin="S" pad="P$2"/>
<connect gate="3" pin="S" pad="P$3"/>
<connect gate="4" pin="S" pad="P$4"/>
<connect gate="5" pin="S" pad="P$5"/>
<connect gate="6" pin="S" pad="P$6"/>
<connect gate="7" pin="S" pad="P$7"/>
<connect gate="8" pin="S" pad="P$8"/>
<connect gate="9" pin="S" pad="P$9"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RJ45" prefix="X">
<description>RJ45, Vertical</description>
<gates>
<gate name="G$1" symbol="JACK8"/>
</gates>
<devices>
<device name="" package="RJ45-VERT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
